	SAFETY DATA SHEET
 

PrimeTec


ACCORDING TO EC-REGULATIONS 1907/2006 (REACH), 1272/2008 (CLP) & 2020/878
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	Date of issue: TBC once finalised
Version 1.0



SECTION 1: IDENTIFICATION OF THE SUBSTANCE/MIXTURE AND OF THE COMPANY/UNDERTAKING
	

	1.1
	Product Identifier

	

	
	Product Name 
	PrimeTec

	
	Product Code

	

	
	Unique Formula Identifier (UFI)

	

	
	Nanoform

	The product does not contain nanoparticles.
	
	
	

	1.2
	Relevant identified uses of the substance or mixture and uses advised against

	Primer for Porcelain Tiles and Natural Stone

	
	Identified use(s)

	A Priming Slurry for Porcelain Tiles and Natural Stone 



	
	Uses advised against

	No Other Uses 

	
	
	

	1.3
	Details of the supplier of the safety data sheet

	

	
	Company Identification

	KelTec Building and Paving Products LTD

	
	
	

	
	Telephone	00-353-(0)53-9233771

	
	Fax	

	
	E-mail (competent person)	Info@keltecltd.ie

	
	
	

	1.4
	Emergency Telephone Number	 

	
	Emergency Phone No.	00-353-(0)53-9233771

	
	Language(s) spoken:	English 


SECTION 2: HAZARDS IDENTIFICATION
	2.1
	Classification of the substance or mixture

	

	
	Regulation (EC) No. 1272/2008 (CLP)

	Skin Irrit. 2; H315
Skin Sens. 1; H317
Eye Dam. 1; H318
STOT SE 3; H335

	
	
	

	2.2
	Label elements 
	According to Regulation (EC) No. 1272/2008 (CLP)


	
	Product name 
	PrimeTec

	
	Contains:

	Cement, portland, chemicals; Flue dust, 

	
	
	

	
	Hazard Pictogram(s)

	[image: ]
	[image: ]
	

	
	
	
	
	

	
	Signal Word(s)

	DANGER
	
	
	

	
	Hazard Statement(s)

	H315: Causes skin irritation.
H317: May cause an allergic skin reaction.
H318: Causes serious eye damage.
H335: May cause respiratory irritation.


	
	
	

	
	Precautionary Statement(s)

	P103: Read label before use.
P102: Keep out of reach of children.
P280: Wear protective gloves/protective clothing/eye protection/face protection/hearing protection.
P302+P352: IF ON SKIN: Wash with plenty of soap and water.
P305+P351+P338: IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.
P310: Immediately call a POISON CENTER/doctor.


	
	
	

	
	Supplemental information

	Not  applicable
	
	
	

	2.3
	Other hazards

	None Known


SECTION 3: COMPOSITION/INFORMATION ON INGREDIENTS
	3.1 
	Substances

	
	Not applicable
	3.2
	Mixtures

	
	

	EC Classification Regulation (EC) No. 1272/2008 (CLP)
	Chemical identity of the substance
	%W/W
	CAS No.
	EC No.
	REACH Registration No.
	Hazard Statement(s)

	Cement, portland, chemicals
	20-40
	65997-15-1
	266-043-4
	Not yet assigned in the supply chain	Skin Irrit. 2; H315
Skin Sens. 1B; H317
Eye Dam. 1; H318
STOT SE 3; H335

	Flue dust, portland cement
	1-2
	68475-76-3
	270-659-9
	01-2119486767-17-0024
	Skin Irrit. 2; H315
Skin Sens. 1; H317
Eye Dam. 1; H318
STOT SE 3; H335




	

	Note: For full text of H phrases see section 16.


SECTION 4: FIRST AID MEASURES
[image: FFAID] 

	4.1
	Description of first aid measures 
	

	
	Self-protection of the first aider
	No action should be taken involving personal risk. Use personal protective equipment as required. Ensure adequate ventilation Avoid inhalation of dusts. Avoid contact with skin and eyes.

	
	Inhalation
	IF INHALED: Remove person to fresh air and keep comfortable for breathing.  In case of respiratory tract irritation, consult a physician.

	
	Skin contact
	IF ON SKIN: Gently wash with plenty of soap and water. If irritation develops and persists, get medical attention.

	
	Eye contact
	IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.  If possible, use isotonic water (0.9% NaCl). After rinsing affected eyes must be seen by an ophthalmologist. Do not rub eyes in order to avoid possible corneal damage by mechanical stress. 

	
	Ingestion
	IF SWALLOWED: Rinse mouth. Give plenty of water to drink. Do NOT induce vomiting. Seek medical treatment.

	4.2
	Most important symptoms and effects, both acute and delayed
	May cause respiratory irritation. May cause an allergic skin reaction. Causes serious eye damage. May cause respiratory irritation.
Handling of this material may generate a dust which can cause mechanical irritation of the eyes, skin nose and throat.

	4.3
	Indication of any immediate medical attention and special treatment needed
	Treat symptomatically.
	
	Notes to a physician:	Treatment by an ophthalmologist due to possible caustic burn of the eyes may be required.

	
	
	Symptoms may be delayed for as long as 48 hours following exposure.

SECTION 5: FIREFIGHTING MEASURES
	5.1
	Extinguishing media
	

	
	Suitable extinguishing media
	Not flammable. In case of fire use extinguishing media appropriate to surrounding conditions. Water spray, foam, dry powder or CO2.

	
	Unsuitable extinguishing media
	Do not use water jet. Direct water jet may spread the fire.

	5.2
	Special hazards arising from the substance or mixture
	May give off noxious and toxic fumes in a fire. Combustion products: Carbon monoxide, Carbon dioxide, Nitrogen oxides (NOx), Metal oxides.

	5.3
	Advice for firefighters
	Fight fire with normal precautions from a reasonable distance. Fire fighters should wear complete protective clothing including self-contained breathing apparatus. Keep containers cool by spraying with water if exposed to fire. Avoid run off to waterways and sewers.


SECTION 6: ACCIDENTAL RELEASE MEASURES
	6.1
	Personal precautions, protective equipment and emergency procedures
	No action should be taken involving personal risk. Wear suitable protective clothing. Ensure adequate ventilation Avoid breathing dust Avoid contact with skin and eyes. Remove contaminated clothing and wash all affected areas with plenty of water. Take precautionary measures against static discharges.

	6.2
	Environmental precautions
	Do not allow to enter drains, sewers or watercourses.

	6.3
	Methods and material for containment and cleaning up
	Take up mechanically, placing in appropriate containers for disposal. A vacuum equipped with HEPA (high efficiency particulate air) filtration is recommended. Treat the recovered material as prescribed in the section on waste disposal.

	6.4
	Reference to other sections
	See Also Section: 8, 13.


SECTION 7: HANDLING AND STORAGE
	7.1
	Precautions for safe handling
	When using do not eat or drink. Wear suitable protective clothing. Provide adequate ventilation when using the material and follow the principles of good occupational hygiene to control personal exposures. Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking. Do not eat, drink or smoke when using this product. Remove contaminated clothing and wash clothing before reuse. Avoid breathing dust. Avoid contact with skin and eyes. Avoid dust generation.

	7.2
	Conditions for safe storage, including any incompatibilities
	Keep only in original packaging. Keep in a well ventilated place. Keep container closed. Take precautionary measures against static discharges.

	
	Storage temperature 
	Ambient temperatures.
	
	Incompatible materials
	When wet: Acids, ammonium salts, aluminium, copper and their alloys.

	7.3
	Specific end use(s)
	See Section: 1.2


SECTION 8: EXPOSURE CONTROLS/PERSONAL PROTECTION
	8.1
	Control parameters
	

	8.1.1
	Occupational exposure limits
	

	

	  
	SUBSTANCE
	CAS No.
	LTEL (8 hr TWA ppm)
	LTEL (8 hr TWA mg/m³)
	STEL (ppm)
	STEL (mg/m³)
	Note

	Cement, portland, chemicals
	65997-15-1
	-
-
	10
4
	-
-
	-
-
	-
-



Source: Health and Safety Authority, Code of Practice, 2020

	

	8.1.2
	Biological limit value
	Not established
	
	
	

	8.1.3
	PNECs and DNELs
	Exposure scenarios for these substances are not yet available in the supply chain
	
	
	

	8.2
	Exposure controls 
	

	8.2.1
	Appropriate engineering controls
	Provide adequate ventilation when using the material and follow the principles of good occupational hygiene to control personal exposures. Take action to prevent static discharges. Keep away from fire, sparks and heated surfaces. Avoid dust generation

	
	
	

	8.2.2
	Individual protection measures, such as personal protective equipment 
	Use personal protective equipment as required. Take care for general good hygiene and housekeeping. Avoid inhalation of vapours that may be evolved at elevated temperatures. Avoid breathing dust. Avoid contact with skin and eyes. Wash hands before breaks and after work. A washing facility/water for eye and skin cleaning purposes should be present.

	
	
	

	Protective clothing should be selected specifically for the working place, depending on concentration and quantity of the hazardous substances handled. The resistance of the protective clothing to chemicals should be ascertained with the respective supplier.

	

	

	Eye/ face protection
[image: 1-EYES]
	Wear eye protection with side protection (EN166). Eyewash bottles should be available.

	
	
	

	
	Skin protection
[image: 1-GLOVES]
	Hand protection: Wear impervious gloves (EN374). Gloves should be changed regularly to avoid permeation problems. 


Body protection: Wear dust-resistant protective clothing.

	
	
	

	
	Respiratory protection
[image: 1-GASMASK]
	Not normally required. Wear suitable respiratory protective equipment if processing involves working in areas where dusts or vapours are likely to be evolved. In case of inadequate ventilation wear respiratory protection. Recommended: EN143 Type A-P2. 

	
	
	

	
	Thermal hazards
	Not applicable

	
	
	

	8.2.3
	Environmental exposure controls
	Avoid release to the environment.


SECTION 9: PHYSICAL AND CHEMICAL PROPERTIES
	9.1
	Information on basic physical and chemical properties 

	
	Physical state

	Powder

	
	Colour                                                                               

	Grey


	
	Odour                                                                                     
	Slight

	
	Melting point/freezing point

	N/A

	
	Boiling point or initial boiling point and boiling range

	N/A

	
	Flammability

	N/A

	
	Lower and upper explosion limit

	N/A

	
	Flash point

	N/A

	
	Auto-ignition temperature

	N/A

	
	Decomposition temperature

	N/A

	
	pH

	N/A

	
	Kinematic viscosity

	N/A

	
	Solubility

	Slightly soluble in water

	
	Partition coefficient: n-octanol/water (log value)
	N/A

	
	Vapour pressure

	N/A

	
	Density and/or relative density

	N/A

	
	Relative vapour density

	N/A

	
	Particle characteristics

	N/A

	
	
	

	9.2
	Other information

	None Known

SECTION 10: STABILITY AND REACTIVITY
	10.1
	Reactivity
	When mixed with water, cements will harden into a stable mass that is not reactive in normal environments
	10.2
	Chemical stability
	Stable under normal conditions

	10.3
	Possibility of hazardous reactions
	Dissolves in hydrofluoric acid to produce corrosive silicon tetrafluoride gas.
	10.4
	Conditions to avoid
	Protect from direct sunlight. Avoid contact with moisture

	10.5
	Incompatible materials
	Incompatible with acids, with ammonium salts and with aluminium, copper and their alloys.
	10.6
	Hazardous decomposition products
	May give off noxious and toxic fumes in a fire. Combustion products: Carbon monoxide, Carbon dioxide


SECTION 11: TOXICOLOGICAL INFORMATION
	11.1
	Information on hazard classes as defined in Regulation (EC) No 1272/2008
	

	
	Acute toxicity - Ingestion
	Mixture: Based upon the available data, the classification criteria are not met.
Calculated acute toxicity estimate (ATE) >2,000 mg/kg.

	
	Acute toxicity - Inhalation
	Mixture: Based upon the available data, the classification criteria are not met.
Calculated acute toxicity estimate (ATE) >2,000 mg/kg.

	
	Acute toxicity - Skin contact
	Mixture: Based upon the available data, the classification criteria are not met.
Calculated acute toxicity estimate (ATE) > 5 mg/L (Dust) 

	
	Skin corrosion/irritation
	Mixture: Skin Irrit. 2; H315: Causes skin irritation.

	
	Flue dust, portland cement
	Skin Irrit. 2; H315: Causes skin irritation.
Irritating to skin. (OECD 431) (Unnamed, 2010)	

	
	Cement, portland, chemicals
	Skin Irrit. 2; H315: Causes skin irritation.
No data available. EU classification and labelling inventory

	
	Serious eye damage/irritation
	Mixture: Eye Dam. 1; H318: Causes serious eye damage.

	
	Flue dust, portland cement
	Eye Dam. 1; H318: Causes serious eye damage.
Irreversible effects on the eye. (OECD 438) (Unnamed, 2010)	

	
	Cement, portland, chemicals
	Eye Dam. 1; H318: Causes serious eye damage.
No data available. EU classification and labelling inventory

	
	Respiratory or skin sensitisation
	Mixture: Skin Sens. 1; H317: May cause an allergic skin reaction.

	
	Flue dust, portland cement
	Skin Sens. 1; H317: May cause an allergic skin reaction.
Adverse effects observed: Sensitising. (Unnamed, 2003)

	
	Cement, portland, chemicals
	Skin Sens. 1B; H317: May cause an allergic skin reaction.
No data available. EU classification and labelling inventory

	
	Germ cell mutagenicity
	Mixture: Based upon the available data, the classification criteria are not met.

	
	Carcinogenicity
	Mixture: Based upon the available data, the classification criteria are not met.

	
	Reproductive toxicity
	Mixture: Based upon the available data, the classification criteria are not met.

	
	STOT - Single Exposure
	Mixture: STOT SE 3; H335: May cause respiratory irritation.

	
	Flue dust, portland cement
	STOT SE 3; H335: May cause respiratory irritation.
ECHA Registration Endpoint summary: Weight of evidence approach
NOAEC (mg/m³): 61.0, 90d (rat) (OECD 413)
LOAEC (mg/m³): 5.09, 90d (rat) (OECD 413)

	
	Cement, portland, chemicals
	STOT SE 3; H335: May cause respiratory irritation.
No data available. EU classification and labelling inventory

	
	STOT - Repeated Exposure
	Mixture: Based upon the available data, the classification criteria are not met.

	
	Aspiration hazard
	Mixture: Based upon the available data, the classification criteria are not met.

	
	
	

	11.2
	Information on other hazards
	

	11.2.1
	Endocrine disrupting properties
	This product does not contain a substance that has endocrine disrupting properties with respect to humans as no components meets the criteria.
	11.2.2
	Other information	None


SECTION 12: ECOLOGICAL INFORMATION
	12.1
	Toxicity
	Mixture: Based upon the available data, the classification criteria are not met. 
LC50: >100 mg/L

	12.2
	Persistence and degradability
	No data for the mixture as a whole.

	
	Flue dust, portland cement
	Not applicable for inorganic substances. 

	
	Cement, portland, chemicals
	Not applicable for inorganic substances. 

	12.3
	Bioaccumulative potential
	No data for the mixture as a whole.

	
	Flue dust, portland cement
	Not applicable for inorganic substances. 

	
	Cement, portland, chemicals
	Not applicable for inorganic substances. 

	12.4
	Mobility in soil
	No data for the mixture as a whole.

	
	Flue dust, portland cement
	Not applicable for inorganic substances. 

	
	Cement, portland, chemicals
	Not applicable for inorganic substances. 

	12.5
	Results of PBT and vPvB assessment
	Not classified as PBT or vPvB.

	12.6
	Endocrine disrupting properties
	This product does not contain a substance that has endocrine disrupting properties with respect to non-target organisms as no components meets the criteria.
	12.7
	Other adverse effects
	None Known


SECTION 13: DISPOSAL CONSIDERATIONS
	13.1
	Waste treatment methods
	Dispose of wastes in an approved waste disposal facility. Recover or recycle if possible.

	
	Waste classification according to Directive 2008/98/EC (Waste Framework Directive)
	HP 4 - Irritant - skin irritation and eye damage


SECTION 14: TRANSPORT INFORMATION
	Not classified according to the United Nations ‘Recommendations on the Transport of Dangerous Goods’.

	
	
	ADR/RID
	ADN	IMDG
	IATA/ICAO

	14.1
	UN number or ID number 

	Not classified
	Not classified
	Not classified
	Not classified

	14.2
	UN proper shipping name
	Not classified
	Not classified
	Not classified
	Not classified

	14.3
	Transport hazard class(es)
	Not classified
	Not classified
	Not classified
	Not classified

	14.4
	Packing group
	Not classified
	Not classified
	Not classified
	Not classified

	14.5
	Environmental hazards
	Not classified
	Not classified
	Not classified
	Not classified

	14.6
	Special precautions for user
	See Section: 2

	14.7
	Maritime transport in bulk according to IMO instruments
	Not applicable

	
	
	

	14.8
	Additional information
	None
	
	
	


SECTION 15: REGULATORY INFORMATION
	15.1
	Safety, health and environmental regulations/legislation specific for the substance or mixture
	

	15.1.1
	EU regulations
	

	
	Authorisations and/or restrictions on use
	Not restricted
	15.1.2
	National regulations
	

	
	Germany
	Water hazard class: Not hazardous (Self classification)

	15.2
	Chemical Safety Assessment
	A REACH chemical safety assessment has not been carried out.

SECTION 16: OTHER INFORMATION
	The following sections contain revisions or new statements: Not  applicable – V1.0

	

	References: 
Existing Safety Data Sheet (SDS) 
Existing ECHA registration(s) for Flue dust, portland cement (CAS No. 68475-76-3).

	

	EU Classification: This Safety Data Sheet was prepared in accordance with EC Regulation (EC) 1907/2006 (REACH), 1272/2008 (CLP) & 2020/878

	

		Classification of the substance or mixture According to Regulation (EC) No. 1272/2008 (CLP)
	Classification procedure

	Skin Irrit. 2; H315
	Additivity method.

	Skin Sens. 1; H317
	Threshold limit.

	Eye Dam. 1; H318
	Additivity method.

	STOT SE 3; H335
	Threshold limit.




	

	Legend

	ADR
	ADR: European Agreement concerning the International Carriage of Dangerous Goods by Road 

	ADN
	ADN: European Agreement on the International Transport of Dangerous Goods by Inland Waterways
	CLP
	Regulation (EC) No 1272/2008 on classification, labelling and packaging of substances and mixtures 

	DNEL
	Derived no effect level

	IATA
	IATA: International Air Transport Association 

	ICAO
	ICAO: International Civil Aviation Organization 

	IMDG
	IMDG: International Maritime Dangerous Goods 

	LTEL
	Long term exposure limit 

	PBT
	PBT: Persistent, Bioaccumulative and Toxic

	PNEC
	Predicted No Effect Concentration

	REACH
	Registration, Evaluation, Authorisation and Restriction of Chemicals

	RID
	RID: Regulations concerning the international railway transport of dangerous goods 

	STEL
	Short term exposure limit

	vPvB
	vPvB: very Persistent and very Bioaccumulative
	
	

	Hazard classification / Classification code:
	Hazard Statement(s)

	Skin irritation, Category 2	H315: Causes skin irritation.
	Serious eye damage, Category 1	H318: Causes serious eye damage.
	Skin sensitizer, Category 1	H317: May cause an allergic skin reaction.
	Skin sensitizer, Sub-category 1B	H317: May cause an allergic skin reaction.
	Specific target organ toxicity (single exposure), Category 3	H335: May cause respiratory irritation.
	
	

	Training advice: Consideration should be given to the work procedures involved and the potential extent of exposure as they may determine whether a higher level of protection is required.

	

	Disclaimers 

	Information contained in this publication or as otherwise supplied to Users is believed to be accurate and is given in good faith, but it is for the Users to satisfy themselves of the suitability of the product for their own particular purpose. Keltec Ltd gives no warranty as to the fitness of the product for any particular purpose and any implied warranty or condition (statutory or otherwise) is excluded except to the extent that exclusion is prevented by law. Keltec Ltd accepts no liability for loss or damage (other than that arising from death or personal injury caused by defective product, if proved), resulting from reliance on this information. Freedom under Patents, Copyright and Designs cannot be assumed.

	

	Annex to the extended Safety Data Sheet (eSDS)

	Exposure scenarios for substances in this preparation are not available.
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